- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Crash Pad / Crash Pad Center Panel Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Crash Pad / Crash Pad Center Panel Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the floor console assembly. (Refer to Floor Console - "Floor Console Assembly")

2. | Remove the crash pad lower panel. (Refer to Crash Pad - "Crash Pad Lower Panel")

3. | Remove the glove box housing. (Refer to Crash Pad - "Glove Box Housing")

4. | After loosening the mounting screws, remove the crash pad center lower panel (A) using a screw driver.

5. | Install in the reverse order of removal.
• | Make sure that the connectors are connected properly.
• | Replace any damaged clips.

##### Crash Pad Center Panel Components and Components Location

Component Location 1. Crash pad center lower panel ...

##### Main Crash Pad Assembly Components and Components Location

Component Location 1. Main crash pad assembly ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Seat Heater (Air Ventilation) Repair procedures

Inspection Front Seat 1. Check for continuity and measure the resistance between terminals. PartConnectorResistance(± 10%)Cushion (C)1-44.54 ?Back (B)1-45.16 ?Set (A)3-49.70 ? Performance of heater is the average temperature of seat surface. The temperatures ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Stabilizer Link Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque : 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft) • Be careful ...
Copyright © www.ksoulev.com 2020-2021