- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: BCM (Body Control Module) / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / BCM (Body Control Module) / Specifications

Specifications

Items | Specifications
Rated voltage | DC 12V
Operating voltage | DC 9 ~ 16V
Operating temperature | -30°C ~ 80°C (-4°F ~ 176°F)
Dark current | BCM & Receiver : Max. 4 mA BCM : Max. 3 mA

##### BCM (Body Control Module)

...

##### Components and Components Location

Components Connector Pin Information No.Connector A (24 pin)Connector B (20 pin)Connector C (26 pin)Connector D (16 pin)1Battery (+)LIN (PAS)Washer motor power-2IGN 1Fuel filler (Charge do ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Temperature Sensor Repair procedures

Inspection High voltage battery heater temperature sensor is installed in modules No. 1 and No. 8. 1. Turn the ignition switch OFF. 2. Shut off the high voltage. (Refer to Battery Control System - "High Voltage Shut-off Procedure") 3. Remove the high volt ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Intake Actuator Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Disconnect the intake actuator connector. 3. Verify that the actuator operates to the recirculation position when 12V is connected to terminal 3 and ground to terminal 7. Verify that the intake actuator operates to the recirculated air posi ...
Copyright © www.ksoulev.com 2020-2021