- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Restraint / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / Repair procedures

Component Replacement after Deployment

Before doing any SRS repairs, use the GDS to check for DTCs. Refer to the Diagnostic Trouble Code list for repairing of the related DTCs.

When the front airbag(s) deployed after a collision, replace the following items.

– | SRSCM

– | Deployed airbag(s)

– | Seat belt pretensioner(s)

– | Emergency fastening device

– | Front impact sensors

– | SRS wiring harnesses

– | Inspect the clock spring for heat damage. If any damage is found, replace the clock spring.

When the side/curtain airbag(s) deployed after a collision, replace the following items.

– | SRSCM

– | Deployed airbag(s)

– | Side impact sensor(s) on the deployed side(s)

– | SRS wiring harnesses

When the vehicle is completely repaired, verify that the SRS airbag system is OK.

– | When the ignition switch is turned ON, the SRS indicator should come on for about 6 seconds before going off.

##### General Safety Information and Caution

Precautions General Precautions Please read the following precautions carefully before performing the airbag system service. Carefully observe the instructions described in this manual as mis ...

##### Airbag Module

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Cooling Duct Repair procedures

Removal Battery Module Outlet Duct • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical in ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components 1. On-Board Charger (OBC)2. Rapid Charge Port3. Normal Charge Port4. High Voltage Battery ...
Copyright © www.ksoulev.com 2020-2021