- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Wiper/Washer / Rear Washer Motor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Rear Wiper/Washer / Rear Washer Motor Repair procedures

Inspection

1. | With the washer motor connected to the reservoir tank, fill the reservoir tank with water.
Before filling the reservoir tank with water, check the filter for foreign material or contamination. if necessary, clean the filter.

2. | Remove the front bumper cover. (Refer to Body - "Front Bumper Cover")

3. | Connect positive (+) and negative (-) battery cables to terminals 1 and 2 respectively to see that the washer motor runs and water is pumped.

4. | Check that the motor operates normally. Replace the motor if it operates abnormally.

##### Rear Washer Switch Repair procedures

Inspection 1. Check for continuity between the terminals while operating the wiper and washer switch. If it is not normal condition, replace wiper and wiper switch. Rear Wiper Switch Rear Wa ...

##### Seat Electrical

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Special Service Tools

Special Service Tools Tool Name / NumberIllustrationDescriptionBand installer09495-3K000Used to install ear type boot bandPuller09495-33000Used to remove spider assemblyBall joint puller09568-34000Used to separate ball joint from the front axle. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Bumper Beam Assembly Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021