- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Door / Rear Door Inside Handle Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Door / Rear Door Inside Handle Repair procedures

Replacement

1. | Remove the rear door trim. (Refer to Rear Door - "Rear Door Trim")

2. | Loosen the rear door inside handle mounting screws (A).

3. | Using a flat-tip screwdriver (B), pull up the rear door inside handle lock pin (C).

4. | Remove the rear door inside handle (A).

5. | Install in the reverse order of removal.
• | Make sure that the door locks/unlocks and opens/closes properly.
• | Replace any damaged clips.

##### Rear Door Trim Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Rear Door Window Glass Components and Components Location

Component Location 1. Rear door window glass ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Charge Port Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be sure ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Wiper Motor Components and Components Location

Component Location 1. Cap2. Nut3. Wiper arm & blade4. Rivet5. Cowl top cover6. Bolt7. Wiper motor & linkage assembly ...
Copyright © www.ksoulev.com 2020-2021