- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Blower / Climate Control Air Filter Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Blower / Climate Control Air Filter Repair procedures

Replacement

1. | Open the glove box (A).

2. | Remove the air filter panel (A).

3. | Remove the filter cover (A) by pressing the filter cover knob.

4. | Replace the air filter (A) with a new one according to the direction of air filter.
• | To remove the filter easily, press the righthand side inward and then pull out the filter.
• | In case of driving in an air-polluted area or rugged terrain, check and replace the air filter as frequently as possible.

5. | Install in the reverse order of removal.

##### Climate Control Air Filter Description and Operation

Description The climate control air filter is located in the blower unit. It eliminates foreign materials and odor. The particle filter performs a role as an odor filter as well as a conventio ...

##### Intake Actuator Description and Operation

Description The intake actuator is located in the blower unit. It regulates the intake door by signal from control unit. Pressing the intake selection switch will shift between recirculation an ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Floor Console Assembly Components and Components Location

Component Location 1. Floor console assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Compressor Oil Repair procedures

Oil Specification 1. The HFC-134a system requires synthetic compressor oil (POE) whereas the R-12 system requires mineral compressor oil. The two oils must never be mixed. 2. Compressor oil (POE) varies according to compressor model. Be sure to use oil specified for the model of compress ...
Copyright © www.ksoulev.com 2020-2021