- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tail Gate / Tail Gate Lift Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Tail Gate / Tail Gate Lift Repair procedures

Replacement

• | Take care to not let the tail gate fall on you as the lifts are removed. Have a helper hold the tail gate open, or use a secure method to hold it open.

1. | Using a screwdriver (A), lift up slightly the socket clips (B) of both ends on the lifter (D), and then remove the lifter from the bracket (C).

2. | Install in the reverse order of removal.
• | Make sure that the tail gate locks and opens properly and locks securely.

##### Tail Gate Back Panel Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Tail Gate Weatherstrip Repair procedures

Replacement 1. Remove the tail gate weatherstrip (A). • Do not apply sealant to the body. 2. Install in the reverse order of removal. & ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Side Weatherstrip Repair procedures

Replacement 1. Loosen the rear door checker (B) mounting bolt. Tightening torque : 16.7 ~ 21.6 N.m (1.7 ~ 2.2 kgf.m, 12.3 ~ 15.9 lb-ft) 2. Detach the clips, then remove the rear door side weatherstrip (A). 3. Install in the reverse order of removal. ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Handling Guide

High voltage battery system inspection guide Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical i ...
Copyright © www.ksoulev.com 2020-2021