- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Crash Pad / Center Fascia Panel Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Crash Pad / Center Fascia Panel Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Using a screwdriver or remover, remove the center fascia panel (A).

2. | Disconnect the A/C & heater controller connectors (A).

3. | Install in the reverse order of removal.
• | Make sure that the connectors are connected properly.
• | Replace any damaged clips.

##### Center Fascia Panel Components and Components Location

Component Location 1. Center fascia panel ...

##### Crash Pad Lower Panel Components and Components Location

Component Location 1. Crash pad lower panel ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Brake Actuation Unit Repair procedures

Removal 1. Turn ignition switch OFF and disconnect the negative (-) battery cable. 2. Disconnect the brake fluid level switch connector (A), and remove the reservoir cap. Be sure to completely remove foreign substances around brake fluid reservoir and cap be ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Troubleshooting

TPMS Inspection method Inspection Find the inspection number by referring to the table above. The following content is irrelevant of the inspection procedure. 1. Warning lamp types • Keeps on without blinking : Low pressure tire warning lamp • ...
Copyright © www.ksoulev.com 2020-2021