- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heating,Ventilation, Air Conditioning / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Specifications

Specification

Air Conditioner

Item | Specification
Compressor | Type | ESC33n (Electric Scroll)
Communication type | CAN communication
Oil type & Capacity | POE OIL, 180±10g
Motor type | BLDC
Rated voltage | 360V
Operation voltage | 240~413V
Displacement | 33cc/rev
Condensor | Heat rejection | 13,400 -3% kcal/hr
Air pressure transducer | Pressure value | Voltage=0.00878835*Pressure(psig)+0.5
Expansion valve | Type | Block type
Refrigerant | Type | R-134a
Capacity | Without heat pump | 550±25g (19.4±0.88 oz.)
With heat pump | 900±25g (31.7±0.88 oz.)

Heater And Evaporator Unit

Item | Specification
PTC Heater | Type | Fin & Tube type
Operating voltage | DC 240V ~ 420V
Heating capacity | 4,700 ± 5% kcal/hr
Heat Pump | Exterior Condensor | Heating capacity | 17,000 - 3% kcal/hr
Interior Condensor | 2,600 - 5% kcal/hr
Chiller | 770g
Accumulator | 950cc
Mode operating type | Actuator
Evaporator | Temperature operating type | Actuator
Temperature contorl type | Evaporator temperature sensor
A/C ON/OFF | ON : 2.3±0.5°C, OFF : 0.6±0.5°C
Heating capacity | 4,700 - 5% kcal/hr

##### High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage syst ...

##### Special Service Tools

Special Service Tools Personal Protective Equipment NameIllustrationDescriptionInsulation glovesUsed when inspecting or working on the high voltage components[Insulation performance : 1000V / ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. BCM & RF receiver2. Key warning switch3. Front door lock actuator & switch4. Rear door lock actuator & switch5. Tailgate open switch ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Curtain Airbag (CAB) Module Description and Operation

Description Curtain airbags are installed inside the headliner (LH and RH) to protect the driver and passenger from danger when side crash occurs. The SRSCM determines deployment of curtain airbag by using side impact sensor (SIS) signal. Never attempt to measu ...
Copyright © www.ksoulev.com 2020-2021