- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Cooling System / Inlet Temperature Sensor Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Cooling System / Inlet Temperature Sensor Description and Operation

Description

Inlet temperature sensor is installed on the No.8 module of high voltage battery and it detects the inner air temperature of battery. The operation of cooling fan depends on the inlet temperature sensor value.

Inlet Temperature Sensor

Installation (on the No.8 battery module)

##### Inlet Temperature Sensor Specifications

Specification Temperature (°C)Resistance (K?)Tolerance (%)-40204.5±4.0-30117.8±3.5- 2070.34±3.0- 1043.43±2.5027.63±2.01018.07±1.62012.11±1.2308.303±1.2405.813±1.5504.149±1.9603.01 ...

##### Inlet Temperature Sensor Schematic Diagrams

Circuit Diagram ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Steering Column Shroud Panel Repair procedures

Replacement [Steering column shroud lower panel] • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Heated Steering wheel Repair procedures

Inspection 1. Measure a resistance of NTC and Heated pad. – NTC resistance(Yellow / Black) - 10k? (9k? ~ 11k?), 25°C – Heated pad resistance (Yellow , Black) - 1.73? ( 2.1 ~ 2.5 ? ) 2. Measure a temperature. – The temperature of wheel surface grip must ris ...
Copyright © www.ksoulev.com 2020-2021