- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / High Voltage Battery Heater Relay Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / High Voltage Battery Heater Relay Specifications

Specification

Item | Specification
ON | Rated Voltage (V) | 450
Rated Current (A) | 10
Voltage Drop (V) | Less than 0.5 (200A)
Coil | Operation Voltage (V) | 12
Resistance (?) | 104.4 ~ 127.6 (20°C)

Item | Specification | Note
Heater Relay Switch Resistance (?) | ? | Checkable by multi tester
Heater Relay Operation Sound | "Clicking" | Checkable by GDS and SST
Heater Relay Coil Resistance (?) | 104.4 ~ 127.6 (20°C) | Checkable by multi tester

##### High Voltage Battery Heater Repair procedures

Inspection When removing the battery pack assembly to inspect the battery system, it can be connected to vehicle by using the SST 0K918-E4100, 0K375-E4100, 0K375-E4 ...

##### High Voltage Battery Heater Relay Components and Components Location

Component 1. Battery Heater2. Battery Heater Relay3. Battery Heater Fuse4. Battery Heater Temperature Sensor ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Windshield Wiper-Washer Switch Repair procedures

Inspection Check for continuity between the terminals while operating the wiper and washer switch. If it is not in normal condition, replace wiper and wiper switch.Wiper Switch Washer Switch Removal 1. Remove the steering column shroud lower / upper panel. (Refer to Body - "Steering Co ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Assembly Components and Components Location

Component Location 1. Front seat assembly ...
Copyright © www.ksoulev.com 2020-2021