- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heat Pump / Accumulator Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Heat Pump / Accumulator Repair procedures

Replacement

1. | Recover the refrigerant with a recovery/ recycling/ charging station.
• | Do not use the same A/C recovery / charging station as conventional belt-driven compressors.
• | Since the electric compressor uses high-voltage, POE oil with high resistivity should be used.
• | If PAG oil mixes into the POE oil of the system, dielectric breakdown may occur due to decreased volumetric resistivity and the A/C compressor may not work.

2. | Disconnect the negative (-) battery terminal.

3. | Remove the refrigerant line after loosening the mounting nuts (A).

4. | Remove the accumulator (A) after loosening the mounting bolt.

5. | Install in the reverse order of removal.
• | Do not use the same A/C recovery / charging station as conventional belt-driven compressors.
• | Since the electric compressor uses high-voltage, POE oil with high resistivity should be used.
• | If PAG oil mixes into the POE oil of the system, dielectric breakdown may occur due to decreased volumetric resistivity and the A/C compressor may not work.

##### Accumulator Description and Operation

Description Separates refrigerant in gas/liquid state so that only the refrigerant in gas state can flow into the compressor. ...

##### Refrigerant Temperature Sensor Components and Components Location

Components Location 1. Refrigerant Temperature Sensor #1 2. Refrigerant Temperature Sensor #2 ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Stabilizer Link Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque : 88.3 ~ 107.9N.m (9.0 ~ 11.0kgf.m, 65.1 ~ 79.6lb-ft) • Be careful ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Radiator Grill Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021