- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Interior Trim / Luggage Side Trim Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Interior Trim / Luggage Side Trim Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the rear seat cushion assembly. (Refer to Rear Seat - "Rear Seat Assembly")

2. | Remove the rear seat back assembly. (Refer to Rear Seat - "Rear Seat Assembly")

3. | Remove the rear door scuff trim. (Refer to Interior Trim - "Door Scuff Trim")

4. | Remove the rear transverse trim. (Refer to Interior Trim - "Rear Transverse Trim")

5. | After loosening the mounting bolts, remove the rear seat lower side bracket (A) [LH,RH].

6. | Carefully remove the rear door body side weatherstrip.

7. | Carefully remove the tail gate weatherstrip.

8. | After loosening the mounting bolt, remove the rear seat belt lower anchir (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.8 ~ 39.8 lb-ft)

9. | After loosening the mounting screw, remove the luggage side trim (A).

10. | Install in the reverse order of removal.
• | Make sure that the connectors are connected in properly.
• | Replace any damaged clips.

##### Luggage Side Trim Components and Components Location

Component Location 1. Luggage side trim ...

##### Rear Pillar Trim Components and Components Location

Component Location 1. Rear pillar trim ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Flex Steer Repair procedures

Replacement 1. Disconnect the negative (-) battery terminal. 2. Remove the driver airbag module. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring") 3. Remove the steering wheel. (Refer to Steering System - "Steering Column and Shaft") 4. Disengage the steering ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Adjustment Glass Adjustment • Check the glass run channels for damage or deterioration, and replace them if necessary. 1. Remove the rear door trim. (Refer to Rear Door - "Rear Door Trim") 2. Remove the rear door window glass mounting hole plug ...
Copyright © www.ksoulev.com 2020-2021