- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Door / Rear Door Belt Outside Weatherstrip Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Door / Rear Door Belt Outside Weatherstrip Repair procedures

Replacement

1. | Pull down rear door window glass by pressing the power window glass switch.

2. | After loosening the mounting screws, remove the rear door belt outside weatherstrip (A).

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Rear Door Latch Repair procedures

Replacement 1. Remove the rear door module. (Refer to Rear Door - "Rear Door Module") 2. Remove the rear door outside handle base (A) by pushing in the lock pins located in the back. 3. ...

##### Rear Door Belt Inside Weatherstrip Repair procedures

Replacement 1. Remove the rear door trim. (Refer to Rear Door - "Rear Door Trim") 2. Remove the rear door belt inside weatherstrip (A). 3. Install in the reverse order of removal. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Schematic Diagrams

Circuit Diagram High Voltage Circuit Diagram ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Tail Gate Assembly Components and Components Location

Component Location 1. Tail gate assembly ...
Copyright © www.ksoulev.com 2020-2021