- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Seat Belt / Rear Seat Belt Retractor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Seat Belt / Rear Seat Belt Retractor Repair procedures

Replacement

• | When installing the belt, be careful not to damage the retractor.

1. | Remove the rear pillar trim. (Refer to Interior Trim - "Rear Pillar Trim")

2. | Loosen the rear seat belt upper anchor (A) mounting bolt.

3. | After loosening the mounting bolt, remove the rear seat belt retractor (B).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.8 ~ 39.8 lb-ft)

4. | Install in the reverse order of removal.
• | Make sure that the connectors are plugged in properly.
• | Replace any damaged clips.

##### Rear Seat Belt Retractor Components and Components Location

Component Location 1. Rear seat belt retractor ...

##### Rear Center Seat Belt Retractor Components and Components Location

Component Location 1. Rear center seat belt retractor ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Horn switch2. Horn relay (EMS box)3. Horn 4. Clock spring ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: TPMS Sensor Description and Operation

Description Mode of Operation ASIC Mode 1. Factory Mode The factory mode is the mode that allows the TPM sensor to transmit RF Frames and sample LF more often in the HKMC factory. The TPM sensor will send normal RF frames in factory mode. LF sampling will occur every 1 second, to ensu ...
Copyright © www.ksoulev.com 2020-2021