- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body (Interior and Exterior) / Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Specifications

Specifications

Items | Specification
Hood | Type | Rear hinged, gas lifter type
Front Door | Structure | Front hinged, frame door Structure
Regulator system | Wire drum type
Locking system | Pin-fork system
Rear Door | Construction | Front hinged, frame door Structure
Regulator system | Wire drum type
Locking system | Pin-fork system
Tail Gate | Type | Front hinged, gas lifter type
Seat Belts | Front | 3 point type with Convertible Locking Retractor (C.L.R)
Rear | 3 point type with Convertible Locking Retractor (C.L.R)

Sealant

Applied parts | Bead width
Panorama Sunroof | Height : 13.5 mm (0.53 in.)
Width : 12 mm (0.47 in.)
Windshield Glass | Height : 12 mm (0.4724 in.)
Width : 8 mm (0.3150 in.)

Tightening Torque

Items | N.m | Kgf.m | lb-ft
Front and rear doors | Door hinge to body | 34.2 ~ 41.2 | 3.5 ~ 4.2 | 25.3 ~ 30.4
Door hinge to door | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Door checker to door | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Door checker to body | 16.7 ~ 21.6 | 1.7 ~ 2.2 | 12.3 ~ 15.9
Door glass mounting bolt | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Outside handle base mounting bolt | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Door channel mounting bolt | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Door channel mounting nut | 3.9 ~ 5.9 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Door latch mounting bolts | 7.8 ~ 10.8 | 0.8 ~ 1.1 | 5.8 ~ 8.0
Door module mounting bolts | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7
Door striker mounting bolts | 16.7 ~ 21.6 | 1.7 ~ 2.2 | 12.3 ~ 15.9
Tail gate | Tail gate hinge to body | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Tail gate hinge to tail gate | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Tail gate latch mounting bolts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Tail gate striker mounting bolts | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood | Hood hinge to body | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood hinge to hood | 21.6 ~ 26.5 | 2.2 ~ 2.7 | 15.9 ~ 19.5
Hood latch to body | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Seat | Front seat mounting bolts | 34.3 ~ 53.9 | 3.5 ~ 5.5 | 25.3 ~ 39.8
Front seat frame mounting bolts | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.8
Rear seat mounting bolts | 16.7 ~ 25.5 | 1.7 ~ 2.6 | 12.3 ~ 18.8
Rear seat latch mounting bolts | 19.6 ~ 29.4 | 2.0 ~ 3.0 | 14.5 ~ 21.7
Seat belt | Height adjuster mounting bolts | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Front seat belt upper anchor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Front seat belt pretensioner mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Rear seat belt retractor mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Rear center seat belt retractor mounting nut | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Seat belt buckle mounting bolt | 39.2 ~ 53.9 | 4.0 ~ 5.5 | 28.9 ~ 39.8
Outside rearview mirror | Outside rearview mirror mounting nuts | 6.9 ~ 10.8 | 0.7 ~ 1.1 | 5.1 ~ 8.0
Wiper arm | Wiper arm mounting nuts | 22.6 ~ 26.5 | 2.3 ~ 2.7 | 16.6 ~ 19.5
Roof rack | Roof rack mounting nuts | 3.9 ~ 4.4 | 0.4 ~ 0.45 | 2.9 ~ 3.3
Quarter fixed glass | Quarter fixed glass mounting nuts | 3.9 ~ 4.4 | 0.4 ~ 0.45 | 2.9 ~ 3.3
Panorama sunroof | Panorama sunroof mounting nuts | 9.8 ~ 14.7 | 1.0 ~ 1.5 | 7.2 ~10.8
Panorama sunroof mounting bolts | 19.6 ~ 29.4 | 2.0 ~ 3.0 | 14.5 ~ 21.7

##### High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage syst ...

##### Special Service Tools

Special Service Tools Tool Name / NumberIllustrationDescriptionHog ring clip installer09880-4F000Used to install hog ring clip Personal Protective Equipment NameIllustrationDescriptionInsu ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Driver Airbag (DAB) Module and Clock Spring Components and Components Location

Components 1. Driver Airbag (DAB)2. Steering Wheel3. Clock Spring ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Power Relay Assembly (PRA) Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be sure ...
Copyright © www.ksoulev.com 2020-2021