- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Bumper / Radiator Grill Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Bumper / Radiator Grill Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the front bumper. (Refer to Front Bumper - "Front Bumper Cover")

2. | Remove the charge door opener cover. (Refer to body -"charge door opener cover" )

3. | Loosen the screws and then remove radiator grill.

4. | Install in the reverse order of removal.
• | Replace the damaged clip.

##### Radiator Grill Components and Components Location

Component Location 1. Radiator grill ...

##### Front Door

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Main Crash Pad Assembly Components and Components Location

Component Location 1. Main crash pad assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Removal 1. Remove the tailgate trim. (Refer to Body - "Tailgate Trim") 2. Remove the tailgate back panel. (Refer to Body - "Tailgate Back Panel") 3. Remove the back view camera (A) after loosening the mounting screws. Installation 1. Install the back view camera. 2. Install th ...
Copyright © www.ksoulev.com 2020-2021