- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Parking Brake System / Electric Parking Brake (EPB) Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Brake System / Parking Brake System / Electric Parking Brake (EPB) Repair procedures

Removal

1. | Turn ignition OFF and disconnect the negative (-) battery cable.

2. | Remove the floor console assembly.(Refer to Body - “Floor console assembly")

3. | Disconnect the EPB control unit mounting nuts and then remove EPB control unit.
Tighten torque: 3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)

4. | Disconnect the EPB control unit connector (A).

Installation

1. | Install in the reverse order of removal.

2. | After replacing the EPB control unit with a new one, “Variant Coding” procedure must be performed.

3. | Perform the “G-Sensor Calibration” with GDS.

4. | Check that the brake operates normally by pushing the EPB switch more than 3 times after installing the EPB module.

Variant coding

1. | Turn ignition "OFF" and connect GDS.

2. | While ignition "ON" & engine "OFF", select vehicle name and EPB system.

3. | Select EPB Variant coding mode.

4. | Perform the "EPB Variant Coding" procedure with GDS.

5. | Complete the “Variant Coding” procedure.

##### Electric Parking Brake (EPB) Schematic Diagrams

EPB Circuit Diagram (1) EPB Circuit Diagram (2) EPB connector input/output Pin DescriptionPin Description1WC-CAN (High)21G/BCenter Fascia Switch (ElectronicParking Brake Switch (SW3 ...

##### EPB Switch Repair procedures

Removal 1. Turn ignition OFF and disconnect the negative (-) battery cable. 2. Remove the floor console upper cover. (Refer to Body group - "Console") 3. Remove the EPB switch assemb ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Relay Specifications

Specification ItemSpecificationONRated Voltage (V)450Rated Current (A)10Voltage Drop (V)Less than 0.5 (200A)CoilOperation Voltage (V)12Resistance (?)104.4 ~ 127.6 (20°C) ItemSpecificationNoteHeater Relay Switch Resistance (?)?Checkable by multi testerHeater Relay Operation Sound"Clickin ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Side Impact Sensor (SIS) Description and Operation

Description Side Impact Sensor (SIS) system consists of two P-SIS, installed at each center of front door modules (LH and RH), and two SIS, installed at each center of nearby pillars (LH and RH). P-SIS or Pressure Side Impact Sensor detects pressure due to collision at its mounting location. ...
Copyright © www.ksoulev.com 2020-2021