- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Crash Pad / Steering Column Shroud Panel Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Crash Pad / Steering Column Shroud Panel Repair procedures

Replacement

[Steering column shroud lower panel]

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the crash pad lower panel. (Refer to Crash Pad - "Crash Pad Lower Panel")

2. | After loosening the mounting screws, remove the steering column shroud lower panel (A) using a screw driver.

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

[Steering column shroud upper panel]

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the cluster fascia panel. (Refer to Crash Pad - "Cluster Fascia Panel")

2. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Steering Column Shroud Panel Components and Components Location

Component Location 1. Steering column shroud lower panel2. Steering column shroud upper panel ...

##### Crash Pad Side Cover Components and Components Location

Component Location [LH] 1. Crash pad side cover [LH] [RH] 1. Crash pad side cover [RH] ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Adjustment Glass Adjustment • Check the glass run channel for damage or deterioration, and replace if necessary. 1. Remove the front door trim. (Refer to Front Door - "Front Door Trim") 2. Remove the front door window glass mounting hole plug (A ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: In-car Sensor Description and Operation

Description The In-car air temperature sensor is integrated into the heater & A/C control unit. The sensor contains a thermistor which measures the temperature of the inside. The signal decided by the resistance value which changes in accordance with perceived inside temperature, is de ...
Copyright © www.ksoulev.com 2020-2021