- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Air Conditioning System / Electric A/C compressor Troubleshooting

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Air Conditioning System / Electric A/C compressor Troubleshooting

Troubleshooting

Fault code | Fail description | Remedy
61 | Compressor CAN signal fault Compressor operation state error receive | 1. Check HV, LV connector connection. 2. Check LV connector pin condition. 3. Check vehicle inverter fuse condition. 4. A/C ON then check compressor operation. 5. If not operating, replace compressor.
62 | Low voltage | 1. Check HV connector connection. 2. Check vehicle inverter fuse condition. 3. Check voltage level of high voltage battery. 4. A/C ON then check compressor operation. 5. If not operating, replace compressor.
63 | High voltage | 1. Identify vehicle model on compressor 2. Check voltage level of high voltage battery. 3. A/C ON then check compressor operation. 4. If not operating, replace compressor.
64 | Overheat protection | 1. Check heating object in engine room. 2. Check A/C system for defects. 3. After 20 minutes, IG ON and A/C ON then check compressor operation. 4. If not operating, replace compressor.
65 | Overloaded | 1. Check cooling fan operation. 2. Check AAF(Active Air Flap) for short circuit 3. After 20 minutes, IG ON and A/C ON then check compressor operation. 4. If not operating, replace compressor.
66 | Over current protection
68 | Missed restart
71 | Failure of Over torque stall
67 | Abnormal (not receiving) | 1. Check 12V battery fuse. 2. Check LV connector connection. 3. Check FATC CAN connection. 4. If not operating, replace compressor.
69 | Failure of thermistor open | 1. Check thermistor condition and inspect.
70 | Failure of thermistor short
72 | Failure of short circuit current | 1. Replace compressor. 2. Check vehicle inverter fuse (if necessary, replace).
73 | Failure of driver voltage
74 | Failure of current measuring
75 | Failure max temperature gradient
76 | Failure Internal Error

##### Electric A/C compressor Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure t ...

##### Condenser Components and Components Location

Component Location [Without Heat Pump] 1. Condenser ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Pre-Charge Registor Specifications

Spectification ItemSpecificationCoilCapacity (W)60Resistance (?)30 ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Transverse Trim Components and Components Location

Component Location 1. Rear transverse trim ...
Copyright © www.ksoulev.com 2020-2021