- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Hood / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Hood / Repair procedures

Adjustment

1. | After loosening the hinge (A) mounting bolt, adjust the hood (B) clearance by moving it up and down, or left and right.

2. | Adjust the hood height by turning the hood overslam bumpers (C).

3. | After loosening the hood latch (D) mounting bolts, adjust the latch by moving it up and down, or left and right.

##### Hood

...

##### Hood Assembly Components and Components Location

Component Location 1. Hood assembly ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Removal • Put on gloves to protect your hands. • Use seat covers to avoid damaging any surfaces. 1. Remove the rear pillar trim. (Refer to Interior Trim - "Rear Pillar Trim") 2. Loosen the quarter fixed g ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Remove engine room under cover. (Refer to Motor System - "Under Cover") 3. Remove the horn (A) after disconnecting the mounting bolt and connector. Installation 1. Install the horns after connecting the horn connectors. ...
Copyright © www.ksoulev.com 2020-2021