- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Parking Brake System / Electric Parking Brake (EPB) Schematic Diagrams

Kia Soul EV (PS EV) 2015-2020 Service Manual / Brake System / Parking Brake System / Electric Parking Brake (EPB) Schematic Diagrams

EPB Circuit Diagram (1)

EPB Circuit Diagram (2)

EPB connector input/output

Pin | Description | Pin | Description
1 | W | C-CAN (High) | 21 | G/B | Center Fascia Switch (ElectronicParking Brake Switch (SW3))
2 | Br | C-CAN (Low) | 22 | - | -
3 | - | - | 23 | - | -
4 | - | - | 24 | - | -
5 | - | - | 25 | - | -
6 | - | - | 26 | - | -
7 | - | - | 27 | G | Center Fascia Switch (ElectronicParking Brake Switch (SW2))
8 | - | - | 28 | - | -
9 | - | - | 29 | G/O | Center Fascia Switch (ElectronicParking Brake Switch (SW4))
10 | - | - | 30 | - | -
11 | - | - | 31 | - | -
12 | - | - | 32 | - | -
13 | - | - | 33 | R | Electronic Parking Brake Actuator LH (-)
14 | - | - | 34 | B | Ground (GF05)
15 | - | - | 35 | B | Ground (GF05)
16 | - | - | 36 | G | Electronic Parking BrakeActuator RH (-)
17 | - | - | 37 | L/R | Electronic Parking BrakeActuator RH (+)
18 | R | Smart Junction Block (Fuse - MODULE 2) | 38 | B | Electronic Parking BrakeActuator LH (+)
19 | W | Center Fascia Switch (ElectronicParking Brake Switch (SW1)) | 39 | W | PCB Block (Fuse - EPB 1)
20 | - | - | 40 | R | PCB Block (Fuse - EPB 2)

##### Electric Parking Brake (EPB) Description and Operation

Description Description of EPB EPB is an electronic parking brake. Unlike existing parking systems that operate by brake pedals or levers, the EPB system sends a signal to the ECU when the dr ...

##### Electric Parking Brake (EPB) Repair procedures

Removal 1. Turn ignition OFF and disconnect the negative (-) battery cable. 2. Remove the floor console assembly.(Refer to Body - “Floor console assembly") 3. Disconnect the EPB contro ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: ON-Board Charger (OBC) Description and Operation

Description In normal charge, the battery is charged through the On-Board Charger (OBC) using external power supply of 220V. On-Board Charger (OBC) is the equipment that charges the high voltage battery of electric vehicle using the 110 ~ 220V AC power. Its maximum output is 6.6 kW and the e ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Seat Latch Components and Components Location

Component Location 1. Rear seat latch assembly ...
Copyright © www.ksoulev.com 2020-2021