- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: ESP(Electronic Stability Program) System / ESP OFF Switch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Brake System / ESP(Electronic Stability Program) System / ESP OFF Switch Repair procedures

Removal

1. | Turn ignition switch OFF and disconnect the negative (-) battery cable.

2. | Remove the crash pad lower panel. (Refer to Body - "Crash Pad Lower Panel")

3. | Remove the lower crash pad switch assembly (A) by pushing it.

4. | Disconnect the connectors (A) from the lower crash pad switch assembly.

5. | Check the continuity between the switch terminals as the ESP OFF switch is engaged.

##### ESP OFF Switch Description and Operation

Description 1. The ESP OFF switch is used by users to turn off the ESP system. 2. The ESP OFF lamp is on when ESP OFF switch is engaged. ...

##### Steering Angle Sensor Description and Operation

Description Installed in MDPS (Motor Driven Power Steering), the Steering Angle Sensor (SAS) sends signals to HECU through CAN communication line. The SAS is used to determine turning directio ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Mode Control Actuator Repair procedures

Inspection 1. Turn the ignition switch OFF. 2. Disconnect the mode control actuator connector. 3. Verify that the mode control actuator operates to the defrost mode when 12V is connected to terminal 3 and ground to terminal 7. Verify that the mode control actuator operates to the vent m ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Flex Steer Repair procedures

Replacement 1. Disconnect the negative (-) battery terminal. 2. Remove the driver airbag module. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring") 3. Remove the steering wheel. (Refer to Steering System - "Steering Column and Shaft") 4. Disengage the steering ...
Copyright © www.ksoulev.com 2020-2021