- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Seat Belt / Front Seat Belt Pretensioner Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Seat Belt / Front Seat Belt Pretensioner Repair procedures

Replacement

• | When installing the belt, make sure not to damage the pretensioner.

1. | Remove the center pillar upper trim. (Refer to Interior Trim - "Center Pillar Trim")

2. | After loosening the mounting bolt, remove the front seat belt upper anchor (A).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.8 ~ 39.8 lb-ft)

3. | After disconnecting the pretensioner connector lock pin, remove the front seat belt pretensioner connector (A), loosen the mounting bolt, and then remove the front seat belt pretensioner (B).
Tightening torque : 39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.8 ~ 39.8 lb-ft)

4. | Install in the reverse order of removal.
• | Make sure that the connectors are plugged in properly.
• | Replace any damaged clips.

##### Front Seat Belt Pretensioner Components and Components Location

Component Location 1. Front seat belt pretensioner ...

##### Height Adjust Components and Components Location

Component Location 1. Height adjust ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Center Seat Belt Retractor Repair procedures

Replacement • When installing the belt, be careful not to damage the retractor. 1. Remove the rear seat back cover [LH]. (Refer to Rear Seat - "Rear Seat Back Cover") 2. After loosening the mounting nut, remove the rear center seat belt retractor ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Troubleshooting

Troubleshooting Trouble SymptomProbable causeRemedyVehicle pulls to one sideScoring of driveshaft ball jointReplaceWear, rattle or scoring of wheel bearingReplaceDefective front suspension and steeringAdjustment or ReplaceVibrationWear, damage or bending of driveshaftReplaceDrive Shaft rattle a ...
Copyright © www.ksoulev.com 2020-2021