- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body (Interior and Exterior) / Troubleshooting

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Troubleshooting

Troubleshooting

Symptom | Possible Cause | Remedy (Refer to page)
Water leaks from panorama sunroof | Deteriorated roof lid weatherstrip | Replace
Excessive roof lid-to-body clearance and improperly fitted weatherstrip | Adjust
Wind noise around panorama sunroof | Loose or deformed deflector, gaps in body work | Retighten adjust or replace
Noise heard when opening/ closing panorama sunroof | Foreign particles lodged in guide rail | Check drive cable and guide rails for foreign particles
Loose guide rails and lid | Retighten
Motor runs but panorama sunroof does not move or moves only partially | Foreign particles lodged in guide rail | Adjust or replace
Incorrect engagement of motor pinion with drive cable
Decrease in motor`s clutch slipping force
Increased panorama sunroof sliding resistance or interference of panorama sunroof with drive cables, weatherstrip, etc. due to maladjustment of panorama sunroof
Noise in motor (clutch slipping noise from motor when panorama sunroof is fully opened or closed is considered normal) | Incorrect engagement of motor pinion with drive cable | Check pinion installation and
Re-tighten motor
Worn out or damaged motor pinion bearing | Replace motor assembly
Worn out or deformed drive cable | Replace
Door glass fails to operate up and down | Incorrect window glass installation | Adjust position
Damaged or faulty regulator arm or regulator | Correct or replace
Door does not open or close completely | Incorrect door installation | Adjust position
Defective door check assembly | Correct or replace
Door hinge requires grease | Apply grease
Hood does not open or close completely | Striker and latch not properly aligned | Adjust
Incorrectly installed hood | Adjust
Incorrect hood bumper height | Adjust
Water leaks through windshield end rear window | Defective seal | Fill with sealant
Defective flange | Correct

##### Special Service Tools

Special Service Tools Tool Name / NumberIllustrationDescriptionHog ring clip installer09880-4F000Used to install hog ring clip Personal Protective Equipment NameIllustrationDescriptionInsu ...

##### Body Side Moulding

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Belt Outside Weatherstrip Repair procedures

Replacement 1. Pull down rear door window glass by pressing the power window glass switch. 2. After loosening the mounting screws, remove the rear door belt outside weatherstrip (A). 3. Install in the reverse order of removal. • Replace any damaged ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Relay Components and Components Location

Component 1. Battery Heater2. Battery Heater Relay3. Battery Heater Fuse4. Battery Heater Temperature Sensor ...
Copyright © www.ksoulev.com 2020-2021