- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Air Conditioning System / A/C Pressure Transducer Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Air Conditioning System / A/C Pressure Transducer Repair procedures

Inspection

1. | Measure the pressure of high pressure line by measuring voltage output between terminals No. 1 and No. 2.

2. | Inspect the voltage value whether it is within the specified range.
Voltage = 0.00878835 * Pressure + 0.5[PSIA]

3. | If the measured voltage value is not within the specification, replace the A/C pressure transducer.

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Recover the refrigerant with a recovery/charging station.
• | If PAG oil mixes into the POE oil of the system, dielectric breakdown may occur due to decreased volumetric resistivity and the A/C compressor may not work.

3. | Disconnect the A/C pressure transducer connector (A).

4. | Remove the A/C pressure transducer (B). [Without Heat Pump] [With Heat Pump]
• | Be careful not to bend the liquid & suction pipe.

5. | Install in the reverse order of removal.
• | When installing, replace it with a new O-ring (A).

##### A/C Pressure Transducer Description and Operation

Description The A/C Pressure Transducer (APT) converts the pressure value of high pressure line into voltage value after measuring it. Engine ECU converts the voltage value to control the cooli ...

##### Evaporator Temperature Sensor Description and Operation

Description The evaporator temperature sensor will detect the evaporator core temperature and interrupt compressor relay power in order to prevent evaporator from freezing by excessive cooling ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Assembly Repair procedures

Replacement 1. Loosen the front seat assembly mounting bolts (A). Tightening torque : 34.3 ~ 53.9N.m (3.5 ~ 5.5kgf.m, 25.3 ~ 39.8lb-ft) [Front] [Rear] 2. Remove the front seat assembly (A). 3. Disconnect the airbag connector (A), seat heater & power seat switch connector (B) ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Alignment Repair procedures

Front wheel alignment When using a commercially available computerized wheel alignment equipment to inspect the front wheel alignment, always position the vehicle on a level surface with the front wheels facing straight ahead. Prior to wheel alignment, steering ...
Copyright © www.ksoulev.com 2020-2021