- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: ESP(Electronic Stability Program) System / Front Wheel Speed Sensor Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Brake System / ESP(Electronic Stability Program) System / Front Wheel Speed Sensor Repair procedures

Removal

1. | Remove the front wheel & tire.
Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft)

2. | Remove the front wheel speed sensor mounting bolt (A).
Tightening torque: 6.9 ~ 10.8 N.m (0.7 ~ 1.1 kgf.m, 5.1 ~ 8.0 lb-ft)

3. | Disconnect the front wheel speed sensor connector (A).

4. | Loosen the mounting bolt (A) and then remove the front wheel speed sensor.
Tightening torque : 8.8 ~ 13.7 N.m (0.9 ~ 1.4 kgf.m, 6.5 ~ 10.1 lb-ft)

5. | Install in the reverse order of removal.

##### Front Wheel Speed Sensor Components and Components Location

Components 1. Front wheel speed sensor2. Front wheel speed sensor connector ...

##### Rear Wheel Speed Sensor Components and Components Location

Components 1. Rear wheel speed sensor 2. Extension cable assembly ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components [A/T] 1. Console rear cover assembly2. Floor console assembly3. EPB switch assembly4. Wiring assembly5. Cup Hold assembly6. Console side pad [LH]7. Console side pad [RH]8. Supplement cup hold9. Ashtray10. Floor console mat11. Console storage box12. Hole cover ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Battery Heater Relay Repair procedures

Inspection • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be su ...
Copyright © www.ksoulev.com 2020-2021