- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Runaway Arresting Device (RAD) Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Runaway Arresting Device (RAD) Description and Operation

Description

RAD is installed on each battery module.
If the high voltage battery is swollen by cell overcharge, RAD cuts the ground of the main relay and the pre-charge relay.
If the cell is overcharged, the switch turns OFF and the vehicle cannot be driven.

RAD

RAD on 10 cells

RAD on 14 cells

RAD Wiring Harness

Operation

Module | Normal | Failure
Current | ON (Connected) | OFF (Cut off)
RAD | - | Switch rise
High Voltage | Normal | Cut off
Phenomenon | Normal | Failure on starting the motor and warning light
Diagram |  |

##### Runaway Arresting Device (RAD) Components and Components Location

Components Location 1. Runaway Arresting Device (RAD)2. Runaway Arresting Device (RAD) Wiring Harness ...

##### Runaway Arresting Device (RAD) Schematic Diagrams

Circuit Diagram ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Components Location 1. Torsion beam axle2. Shock absorber3. Coil spring assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Air Ventilation Seat Control Unit Components and Components Location

Component Location 1. Seat back blower2. Seat cushion blower3. Air ventilation seat control unit ...
Copyright © www.ksoulev.com 2020-2021