- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Steering wheel / Flex Steer Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Steering System / Steering wheel / Flex Steer Description and Operation

Instruction

Flex Steer is system to choose the three modes power steering depending on driver preference or driving conditions.

• | Display on the cluster but power steering is would not changed while operating the steering wheel.
As a safety measures, mode is changed automatically when steering wheel operation is done.
• | Be sure to carefully change the mode while driving.
• | Electric Power Steering (EPS) is not working due tofailure, "flex steer" may not work.

How to operate

• | First input : Display the current mode on cluster. (4 seconds)

• | Add input (4 seconds) : Mode is changed sequentially.

• | Three steering modes

COMFORT : For the elder and the female drivers: it is mainly used for city driving and stop & parking, and a little lighter power steering.
NORMAL : Basic mode
SPORT : It is mainly used for highway driving, and a little heavy power steering.

##### Flex Steer Components and Components Location

Components Location 1. Flex steering swithch ...

##### Flex Steer Repair procedures

Replacement 1. Disconnect the negative (-) battery terminal. 2. Remove the driver airbag module. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring") 3. Remove the steer ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Smart Key Unit Repair procedures

Inspection Smart Key Unit – Refer to Smart key System - "Smart key Diagnostic" Smart Key Switch – Refer to Smart key System - "Smart key Diagnostic" Antenna – Refer to Smart key System - "Smart key Diagnostic" Trunk Lid Open Switch 1. Check for continuity ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Safety Plug Schematic Diagrams

System Circuit Diagram Circuit Diagram ...
Copyright © www.ksoulev.com 2020-2021