- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tail Gate / Tail Gate Latch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Tail Gate / Tail Gate Latch Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Take care not to scratch the body surface.

1. | Remove the tail gate trim. (Refer to Tail Gate - "Tail Gate Trim")

2. | After loosening the mounting bolts, remove the tail gate latch assembly (A).
Tightening torque : 6.9~10.8 N.m (0.7~1.1 kgf.m, 5.1~8.0 lb-ft)

3. | Disconnect the tail gate latch connector (A).

4. | Install in the reverse order of removal.
• | Make sure that the tail gate locks/unlocks and opens/closes properly.
• | Adjust the tail gate alignment.
• | Make sure that the connectors are connected properly.

##### Tail Gate Latch Components and Components Location

Component Location 1. Tail gate latch assembly ...

##### Tail Gate Back Panel Components and Components Location

Component Location 1. Tail gate back panel ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Console Cover Components and Components Location

Component Location 1. Rear console cover ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Power Relay Assembly (PRA) Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be sure ...
Copyright © www.ksoulev.com 2020-2021