- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Crash Pad / Cluster Fascia Panel Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Crash Pad / Cluster Fascia Panel Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Lower the steering wheel.

2. | Using a screwdriver or remover, remove the cluster fascia panel (A).

3. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Cluster Fascia Panel Components and Components Location

Component Location 1. Cluster fascia panel ...

##### Center Fascia Panel Components and Components Location

Component Location 1. Center fascia panel ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Panorama sunroof2. Panorama sunroof switch3. Panorama sunroof motor & controller4. Roller blind motor & slave controller ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Disc Brakes and Pads Repair procedures

Inspection Check the pads for excessive wear, discs for run out and wear, and calipers for fluid leakage. Front Brake Front Brake Disc Thickness Check 1. Check the brake pads for wear and fade. 2. Check the brake disc for damage and cracks. 3. Remove all rust and contamination fro ...
Copyright © www.ksoulev.com 2020-2021