- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Lift And Support Points / General Information

Kia Soul EV (PS EV) 2015-2020 Service Manual / General Information / Lift And Support Points / General Information

Lift And Support Points

When heavy rear components such as suspension, fuel tank, spare tire, tailgate and trunk lid are to be removed, place additional weight in the luggage area before hoisting. When substantial weight is removed from the rear of the vehicle, the center of gravity may change and can cause the vehicle to tip forward on the hoist.

• | Since each tire/wheel assembly weights approximately 14kg (30lbs), placing the front wheels in the luggage area can assist with the weight distribution.
• | Use the same support points to support the vehicle on safety stands.

1. | Place the lift blocks under the support points as shown in the illustration.

2. | Raise the hoist a few inches (centimeters) and rock the vehicle to be sure it is firmly supported.

3. | Raise the hoist to full height to inspect the lift points for secure support.

##### Lift And Support Points

...

##### Important Safety Notice

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Glass Repair procedures

Removal • In order to remove the rear glass, use the tools shown in the following figure: [Tooling Diagram] Square wire Insert-type wire grip [Tooling Assembly Diagram] • Insert and affix square wire into the insert hole of the wire grip . ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Specifications

Specification ItemSpecificationRated voltageDC 3VOperating voltageDC 2.7V ~ 3.3VOperating temperature-20°C ~ +60°C (-4°F ~ +140°F)RF ModulationFSKLF ModulationASKRF frequency433.92 MHzBatteryCR2032 (3V / 1EA)Transmissible distance30m or moreBattery lifetime2 years or more (at 20 times per d ...
Copyright © www.ksoulev.com 2020-2021