- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Keyless Entry / Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Keyless Entry / Repair procedures

Inspection

Front Door Lock Module Inspection

1. | Remove the front door trim. (Refer to Body - "Front Door Trim")

2. | Remove the front door module. (Refer to Body - "Front Door Module")

3. | Disconnect the connectors from the actuator.

4. | Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily. [Central Lock]

5. | Check for continuity between the terminals in each switch position according to the table.

Rear Door Lock Module Inspection

1. | Remove the rear door trim. (Refer to Body - "Rear Door Trim")

2. | Remove the rear door module. (Refer to Body - "Rear Door Module")

3. | Disconnect the connectors from the actuator.

4. | Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily. [Central Lock]

5. | Check for continuity between the terminals in each switch position according to the table.

Tailgate Lock Module Inspection

1. | Remove the tailgate trim. (Refer to Body - "Tailgate Trim")

2. | Disconnect the 4P connector from the actuator.

3. | Check actuator operation by connecting power and ground according to the table. To prevent damage to the actuator, apply battery voltage only momentarily.

Tailgate Open Switch

1. | Remove the tailgate trim. (Refer to Body - "Tailgate Trim")

2. | Disconnect the connector from the actuator.

3. | Check for continuity between the terminals in each switch position according to the table.

##### Components and Components Location

Component Location 1. BCM & RF receiver2. Key warning switch3. Front door lock actuator & switch4. Rear door lock actuator & switch5. Tailgate open switch ...

##### Lighting System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Yaw-rate and Lateral G Sensor Description and Operation

Description The yaw rate and G sensor is included inside the air bag control module (SRSCM). When the vehicle is turning with respect to a vertical axis the yaw rate sensor detects the yaw rate electronically by the vibration change of plate fork inside the yaw rate sensor. If yaw velocity ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Audio unit2. Tweeter speaker3. Roof antenna4. Front door speaker5. Rear door speaker6. Center speaker7. Antenna cable connector8. Antenna feeder cable ...
Copyright © www.ksoulev.com 2020-2021