- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: SRSCM / Front Impact Sensor (FIS) Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / SRSCM / Front Impact Sensor (FIS) Repair procedures

Removal

• | Removal of the airbag must be performed according to the precautions / procedures described previously.
• | Before disconnecting the front impact sensor connector, disconnect the front airbag connector(s).
• | Do not turn the ignition switch ON nor connect the battery cable while replacing the front impact sensor.

1. | Disconnect the battery negative cable and wait for at least thirty seconds before beginning to work.

2. | Disconnect the front impact sensor connector (A).

3. | Loosen the mounting bolt and then remove the front impact sensor (B) and extension harness.

Installation

• | Do not turn the ignition switch ON nor connect the battery cable while replacing the front impact sensor.

1. | Install the new front impact sensor.

2. | Tighten the front impact sensor (B) mounting bolt.
Tightening torque : 7.8 ~ 9.8 N.m (0.8 ~ 1.0 kgf.m, 5.7 ~ 7.3 lb-ft)

3. | Connect the front impact sensor connector (A).

4. | Reconnect the battery negative cable.

5. | After installing the Front Impact Sensor, confirm proper system operation:
• | Turn the ignition switch ON the SRS indicator light should be turned on for about six seconds and then go off.

##### Front Impact Sensor (FIS) Components and Components Location

Components ...

##### Side Impact Sensor (SIS) Description and Operation

Description Side Impact Sensor (SIS) system consists of two P-SIS, installed at each center of front door modules (LH and RH), and two SIS, installed at each center of nearby pillars (LH and RH ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Door Window Glass Components and Components Location

Component Location 1. Rear door window glass ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High voltage joint box Description and Operation

Description Function: The high voltage joint box distribute high voltage to the each unit of vehicle. High-voltage power charge / output system flow ...
Copyright © www.ksoulev.com 2020-2021