- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: VESS(Virtual Engine Sound System) / Virtual Engine Sound Speaker Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / VESS(Virtual Engine Sound System) / Virtual Engine Sound Speaker Repair procedures

Removal

1. | Disconnect the negative(-) battery terminal.

2. | Remove the front wheel guard. (Refer to Body - "Front Bumper")

3. | Disconnect the VESS connector (A).

4. | Remove the VESS speaker (A) after loosening the mounting bolts.

Installation

1. | Install the VESS speaker and connector.

2. | Install the front wheel guard.

3. | Connect the negative (-) battery terminal.

##### Virtual Engine Sound Speaker Components and Components Location

Component Location ...

##### Windshield Wiper/Washer

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Inlet Temperature Sensor Description and Operation

Description Inlet temperature sensor is installed on the No.8 module of high voltage battery and it detects the inner air temperature of battery. The operation of cooling fan depends on the inlet temperature sensor value. Inlet Temperature Sensor Installation (on the No.8 battery modu ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Removal • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. • Be sure ...
Copyright © www.ksoulev.com 2020-2021