- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Front Door / Front Door Outside Handle Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Front Door / Front Door Outside Handle Repair procedures

Replacement

1. | Remove the hole plug (A).

2. | After loosening the mounting bolt, remove the front door outside handle cover (B).
Tightening torque : 7.8 ~ 11.8 N.m (0.8 ~ 1.2 kgf.m, 5.8 ~ 8.7 lb-ft)

3. | Remove the front door outside handle (A) by sliding it backward.

4. | Disconnect the front door outside handle connector (A).

5. | Install in the reverse order of removal.
• | Be sure to install the outside handle pad (A) between the outside handle and the door panel.
• | Make sure that the connectors are connected properly.
• | Make sure that the door locks/unlocks and opens/closes properly.

##### Front Door Outside Handle Components and Components Location

Component Location 1. Front door outside handle ...

##### Front Door Latch Components and Components Location

Component Location 1. Front door latch ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Schematic Diagrams

Circuit Diagram Connector Pin Information No.Wire harness connectorPanorama motorBlind motor1Ground 1Ground 1Ground 22Glass status signal / Tool glassGlass status signal/ Tool (Parameter)Tool (Parameter)3IGN 2IGN 2-4Up switchUp switch-5---6Battery 1Battery 1Battery 27Ground 2SerialSerial8Vehic ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Rear Coil Spring Components and Components Location

Components 1. Spring lower pad2. Spring3. Spring upper pad ...
Copyright © www.ksoulev.com 2020-2021