- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Lighting System / Troubleshooting

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Lighting System / Troubleshooting

Troubleshooting

Symptom | Possible cause | Remedy
Only one lamp lights on (All exterior lamps) | Bulb burned out | Replace bulb
Socket, wiring or ground faulty | Repair if necessary
Head lamps do not light on | Bulb burned out | Replace bulb
Ignition fuse (LOW:10A, HIGH:20A) blown | Check for short and replace fuse
Head lamp fuse (15A) blown | Check for short and replace fuse
Head lamp relay faulty | Check relay
Lighting switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Tail lamps and license plate lamp do not light on | Bulb burned out | Replace bulb
Tail lamp fuse (10A) blown | Check for short and replace fuse
Tail lamp relay faulty | Check relay
Lighting switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Stop lamps do not light on | Bulb burned out | Replace bulb
Stop lamp fuse (15A) blown | Check for short and replace fuse
Stop lamp switch faulty | Adjust or replace switch
Wiring or ground faulty | Repair if necessary
Stop lamps do not turn off | Stop lamp switch faulty | Repair or replace switch
Instrument lamps do not light on (Tail lamps light on) | Rheostat faulty | Check rheostat
Wiring or ground faulty | Repair if necessary
Turn signal lamp flashes only on one side | Bulb burned out | Replace bulb
Turn signal switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Turn signal lamps do not light on | Bulb burned out | Replace bulb
Turn signal lamp fuse (10A) blown | Check for short and replace fuse
Flasher unit faulty | Check flasher unit
Turn signal switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Hazard warning lamps do not light on | Bulb burned out | Replace bulb
Hazard warning lamp fuse (15A) blown | Check for short and replace fuse
Flasher unit faulty | Check flasher unit
Hazard switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Flasher rate too slow or too fast | Lamps'' wattages are smaller or larger than specified | Replace lamps
Flasher unit faulty | Check flasher unit
Back up lamps do not light on | Bulb burned out | Replace bulb
Back up lamp fuse (10A) blown | Check for short and replace fuse
Back up lamp switch (M/T) faulty | Check switch
Transaxle range switch (A/T) faulty | Check switch
Wiring or ground faulty | Repair if necessary
Room lamp does not light on | Bulb burned out | Replace bulb
Room lamp fuse (10A) blown | Check for short and replace fuse
Room lamp switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Front fog lamps do not light on | Bulb burned out | Replace bulb
Front fog lamp fuse (15A) blown | Check for short and replace fuse
Front fog lamp relay faulty | Check relay
Front fog lamp switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Wiring or ground faulty | Repair if necessary
Map lamp does not light on | Bulb burned out | Replace bulb
Room lamp fuse (10A) blown | Check for short and replace fuse
Map lamp switch faulty | Check switch
Wiring or ground faulty | Repair if necessary
Trunk room lamp does not light on | Bulb burned out | Replace bulb
Room lamp fuse (10A) blown | Check for short and replace fuse
Trunk room lamp switch faulty | Check switch
Wiring or ground faulty | Repair if necessary

##### Charge Information Lamp Repair procedures

Removal 1. Disconnect the negative (-) battery terminal. 2. Using the flat screw driver or remover, remove the crash pad center air vent panel (A). 3. Disconnect the hazard switch connecto ...

##### Multifunction Switch

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High voltage joint box Components and Components Location

Components Location 1. High voltage joint box2. Air conditioning compressor high voltage connector3. Electric power control unit (EPCU) high voltage cable4. On-board charger (OBC) high voltage cable connector5. PTC heater high voltage cable6. High voltage battery assembly high voltage cable7. H ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Repair procedures

Component Replacement after Deployment Before doing any SRS repairs, use the GDS to check for DTCs. Refer to the Diagnostic Trouble Code list for repairing of the related DTCs. When the front airbag(s) deployed after a collision, replace the following items. ...
Copyright © www.ksoulev.com 2020-2021