- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Battery Temperature Sensor Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Battery Temperature Sensor Specifications

Specification

Temperature (°C) | Resistance (K?) | Tolerance (%)
-40 | 204.5 | ±4.0
-30 | 117.8 | ±3.5
- 20 | 70.34 | ±3.0
- 10 | 43.43 | ±2.5
0 | 27.63 | ±2.0
10 | 18.07 | ±1.6
20 | 12.11 | ±1.2
30 | 8.303 | ±1.2
40 | 5.813 | ±1.5
50 | 4.149 | ±1.9
60 | 3.013 | ±2.2
70 | 2.225 | ±2.5

##### Main Fuse Repair procedures

Inspection • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failur ...

##### Battery Temperature Sensor Description and Operation

Description Installed in the high voltage battery module, Battery Temperature Sensor transfers temperature of each battery module to BMS ECU. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Battery Management System (BMS) ECU Schematic Diagrams

System Circuit Diagram Connector Location BMS ECU Connector And Terminal Function BMS ECU Terminal Function A Connector [B01-A] (35 Pin) - Voltage Measurement Connector Pin no.DescriptionConnected to1Battery Cell [Module 8/Cell 13] Voltage InputBattery Cell [Module 8/Cell 13]2Battery Cell ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Roof Trim Assembly Components and Components Location

Component Location 1. Roof Trim Assembly ...
Copyright © www.ksoulev.com 2020-2021