- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heater / Temperature Control Actuator Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Heater / Temperature Control Actuator Repair procedures

Inspection

1. | Turn the ignition switch OFF.

2. | Disconnect the temperature control actuator connector.

3. | Verify that the temperature control actuator operates to the cool position when 12V is connected to terminal 3 and ground to terminal 7. Verify that the temperature control actuator operates to the warm position when connected in reverse.
1. - 2. - 3. Cool position 4. Sensor (+ 5V) | 5. Feedback signal 6. Sensor ground 7. Warm position

4. | Connect the temperature control actuator connector.

5. | Turn the ignition switch ON.

6. | Check the voltage between terminals 5 and 4. Specification
Door Position | Voltage (V) | Error Detecting
Max. cooling | 0.3±0.15 | Low voltage : 0.1V or less High voltage : 4.9V or more
Max. heating | 4.7±0.15
It will feedback the current position of the actuator to controls.

7. | If the temperature control actuator does not operate well, substitute with a known-good temperaturecontrol actuator and check for proper operation. Use the replaced actuator if it performs well.

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the crash pad lower panel. (Refer to Body - "Crash Pad Lower Panel")

3. | Remove the driver''s side shower duct (A) after loosening the screw.

4. | Disconnect the connector (A) and then remove the temperature control actuator (B) after loosening the mounting screws.

5. | Install in the reverse order of removal.

##### Temperature Control Actuator Description and Operation

Description The heater unit includes mode control actuator and temperature control actuator. Located in the heater unit, the temperature control actuator regulates the temperature in the following ...

##### Mode Control Actuator Description and Operation

Description Located in the heater unit, the mode control actuator adjusts the position of the mode door by operating the mode control actuator according to the signal from the A/C control unit. ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Outside Rear View Mirror Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Ta ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage Shut-off Procedures

High Voltage Shut-off Procedure Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failure to follow the safety instructions may result in serious electrical injuries. ...
Copyright © www.ksoulev.com 2020-2021