- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Lighting System / Hazard Lamp Switch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Lighting System / Hazard Lamp Switch Repair procedures

Inspection

1. | The SJB can be diagnosed by using the GDS. The SJB communicates with the GDS which then displays inputs and outputs along with codes. It will be able to quickly diagnose defects of hazard lamp switch with GDS. GDS can forcefully operate actuator, monitor input/output values and self diagnose.

2. | To diagnose the SJB function, select the vehicle model, BCM and SJB.

3. | To consult the present input/output values of SJB, select "Current DATA" to view current information of SJB input/output conditions.

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the center airvent assembly (A).

3. | Disconnect the connector (A) from the center airvent assembly.

4. | Remove the hazard switch (A) from the center airvent assembly.

Installation

1. | Install the hazard switch in the center airvent assembly.

2. | Connect the connector and install the center airvent assembly.

3. | Connect the negative (-) battery terminal.

##### Overhead Console Lamp Repair procedures

Inspection 1. Remove the overhead console lamp assembly then check for continuity between terminals. If the continuity is not as specified, replace the map lamp switch. No.Description1Groun ...

##### Rheostat Repair procedures

Inspection 1. Disconnect the negative (-) battery terminal. 2. Remove the crash pad lower panel. (Refer to Body - "Crash Pad Lower Panel") 3. Remove the lower crash pad switch assembly (A ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Panorama Sunroof Switch Repair procedures

Inspection 1. Disconnect the negative (-) battery terminal. 2. Open the sunglass case cover from the overhead console then remove the 2 screws holding the overhead console. Disconnect the switch connector and Map lamp connector, and then remove the overhead console lamp (A). 3. Che ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component High Voltage Battery 1. Cooling Fan2. Outlet Cooling Duct3. Protector Outlet Duct Panel4. Battery Module Outlet Duct5. Inlet Temperature Sensor Vehicle 1. Cooling Fan Relay ...
Copyright © www.ksoulev.com 2020-2021