- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: SRSCM / Side Impact Sensor (SIS) Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Restraint / SRSCM / Side Impact Sensor (SIS) Description and Operation

Description

Side Impact Sensor (SIS) system consists of two P-SIS, installed at each center of front door modules (LH and RH), and two SIS, installed at each center of nearby pillars (LH and RH).
P-SIS or Pressure Side Impact Sensor detects pressure due to collision at its mounting location..
Side Impact Sensor is also called A-SIS as it detects acceleration.
SRSCM determines the deployment of airbag and the time of deployment based on the collision signal from the SIS at the time of collision.

##### Front Impact Sensor (FIS) Repair procedures

Removal • Removal of the airbag must be performed according to the precautions / procedures described previously. • Before disconnecting the front ...

##### Side Impact Sensor (SIS) Components and Components Location

Components ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Description System Overview The System offers the following features: – Human machine interface through a 1-stage button, for terminal switching and engine start. – Control of external relays for ACC / IGN1 / IGN2 terminal switching and STARTER, without use of mechanical i ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Luggage Side Trim Components and Components Location

Component Location 1. Luggage side trim ...
Copyright © www.ksoulev.com 2020-2021