- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Rear Bumper / Rear Bumper Beam Assembly Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Rear Bumper / Rear Bumper Beam Assembly Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Use a plastic panel removal tool to remove interior trim pieces to protect from marring the surface.
• | Take care not to bend or scratch the trim and panels.

1. | Remove the rear bumper cover. (Refer to Rear Bumper - "Rear Bumper Cover")

2. | Disconnect the bumper antenna connector (A) and license lamp connector (B).

3. | Remove the joint connector mounting clip (C).

4. | Remove the rear bumper wiring harness mounting clips (A).

5. | Remove the mounting clips (B) and the rear bumper beam assembly (C), and then loosen the clips.

6. | Install in the reverse order of removal.
• | Make sure that the connectors are plugged in properly.
• | Replace any damaged clips.

##### Rear Bumper Beam Assembly Components and Components Location

Component Location 1. Rear bumper beam assembly ...

##### Rear Door

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Quick Charge Specifications

Specification Output 100kWDC 500V, 200A50kWDC 450V, 110A ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Outer Condenser Components and Components Location

Components Location 1. Outer Condenser ...
Copyright © www.ksoulev.com 2020-2021