- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Electro Chromic Inside Rear View Mirror / Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Electro Chromic Inside Rear View Mirror / Description and Operation

Description

The Electro Chromatic inside rear view Mirror (ECM) is intended to dim the reflecting light in the rear view mirror. The forward facing sensor detects the brightness of the surroundings while the rearward looking sensor detects the intensity of the light from the rear. The intensity of the light from the rear sensor is used by the mirror to adjust the level of shading ranging from 7% to 85%. When the reverse gear is engaged, it stops functioning.

1. | The forward facing sensor sees if the brightness of the surroundings is low enough for the mirror to operate its function.

2. | The rearward looking sensor detects glaring of the reflecting light from a vehicle behind.

3. | The ECM is darkened to the level as determined by the rearward looking sensor. When the glaring is no longer detected, the mirror stops functioning. (1. LED indicator , 2. ON/OFF Switch , 3. Rearward looking sensor , 4. Forward looking sensor )

Automatic-dimming Function

To protect your vision during nighttime driving, your mirror will automatically dim upon detecting glare from the vehicles traveling behind you. The auto-dimming function can be controlled by the Dimming ON/OFF Button :

1. | Pressing and holding the Feature Control button for more than 3 but less than 6 seconds turns the auto-dimming function OFF which is indicated by the green Status Indicator LED turning off.

2. | Pressing and holding the Feature Control button again for more than 3 but less than 6 seconds turns the auto-dimming function ON which is indicated by the green Status Indicator LED turning on.
The mirror defaults to the "ON" position each time the vehicle is started.

##### Components and Components Location

Components ...

##### Repair procedures

Inspection Check the functions of the ECM in the following procedures: 1. Turn the ignition key to the "ON" position. 2. Cover the forward facing sensor. 3. Flash a light onto the rearwar ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Description Electric vehicle can be charged by two methods, rapid charge and normal charge. In the case of normal charge, the battery is charged after 220V AC power is transformed to DC power by On-Board Charger (OBC). In the case of rapid charge, the DC power from charging station goes di ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: A Pillar Garnish Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Ta ...
Copyright © www.ksoulev.com 2020-2021