- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Fuses And Relays / Relay Box (Passenger Compartment) Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body Electrical System / Fuses And Relays / Relay Box (Passenger Compartment) Repair procedures

Fuse Inspection

1. | Be sure that there are no loose fuse holders and that the fuses are held securely.

2. | Is the fuse capacity correct for each circuit?

3. | Are there any blown fuses? If a fuse is to be replaced, be sure to use a new fuse of the same capacity. At all times, determine the cause of blown fuse and eliminate the problem before installing a new fuse.

Inspection

1. | The SJB can be diagnosed by using the GDS. The SJB communicates with the GDS which then displays inputs and outputs along with codes.

2. | To diagnose the SJB function, select the vehicle model, BCM and SJB.

3. | To consult the present input/output values of SJB, select "Current DATA". It provides information on SJB input/output conditions.

4. | To perform functional test on SJB outputs, select "Actuation Test"

Removal

Passenger Compartment Junction Box (SJB)

1. | Disconnect the negative(-) battery terminal.

2. | Remove the crash pad lower panel. (Refer to Body - "Crash Pad Lower Panel")

3. | Disconnect the connectors from the fuse side of the smart junction box.

4. | Remove the smart junction box (A) after loosening the mounting nuts and bolt.

5. | Disconnect the connectors from the back side of the smart junction box.

Installation

1. | Install the smart junction box.

2. | Install the crash pad lower panel.

3. | Check that all systems operate normally.

##### Relay Box (Passenger Compartment) Description and Operation

Description Smart Junction Box(SJB) 1. General function : Interior Junction Box + some functions of BCM It uses CAN communication and IPS to control loads. 2. Main functions: – Low ...

##### ICM (Integrated Circuit Module) Relay Box Components and Components Location

Component ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Troubleshooting

Troubleshooting Vehicle inspection SYMPTOM CHART SymptomSuspect AreaRemedy (See page)Squeak or grunt-noise from the front suspension, occurs more in cold ambient temperatures-more noticeable over rough roads or when turningFront stabilizer barUnder these conditions, the noise is acceptabl ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Passenger Airbag (PAB) Module Description and Operation

Description Passenger Airbag (PAB) module is located in the passenger crash pad. The PAB contains 2 firing squibs of airbag and 1 firing squib of active vent. The deployment timing of both 2 firing squibs of airbag and 1 firing squib of active vent depends on the crash speed or the level ...
Copyright © www.ksoulev.com 2020-2021