- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Heater / High Voltage PTC Heater Description and Operation

Kia Soul EV (PS EV) 2015-2020 Service Manual / Heating,Ventilation, Air Conditioning / Heater / High Voltage PTC Heater Description and Operation

Operation Condition

1. | The power supplied to the PTC heater should be within DC 240V - 420V (high voltage).

2. | The power supplied to the PTC heater should be within 9.0V - 16.0V (low voltage).

3. | The interlcok and insulation resistance must be normal.

4. | The engine must be running.

5. | The high voltage PTC heater operates depending on the operating Duty output.

6. | If the high voltage PTC heater is abnormal, check the Fail Safe.

##### Evaporator Core Repair procedures

Replacement • Be sure to read and follow the “General Safety Information and Caution” before doing any work related with the high voltage system. Failu ...

##### High Voltage PTC Heater Repair procedures

Inspection 1. Check for output signal in the heater and A/C control unit. 2. Using the GDS, check whether there is a problem in the interlock. 3. Check whether the low voltage (12V) is sup ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Seat Frame Assembly Components and Components Location

Component Location 1. Front seat back frame assembly2. Front seat cushion frame assembly ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: High Voltage PTC Heater Repair procedures

Inspection 1. Check for output signal in the heater and A/C control unit. 2. Using the GDS, check whether there is a problem in the interlock. 3. Check whether the low voltage (12V) is supplied or not. 4. For inspection, refer to the Self Diagnosis and Fail Safe. Replacement ...
Copyright © www.ksoulev.com 2020-2021