- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Battery Management System (BMS) ECU Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Battery Management System (BMS) ECU Specifications

Specification

Item | Specification | Remark
C-CAN terminating resistance (?) | Approx. 60 | Combined resistance (BMS ECU-Inverter)
C-CAN terminating resistnace (?) | Approx. 120 | BMS ECU resistance

##### Inspection

Inspection When removing the battery pack assembly to inspect the battery system, it can be connected to vehicle by using the SST 0K918-E4100, 0K375-E4100, 0K375-E4 ...

##### Battery Management System (BMS) ECU Schematic Diagrams

System Circuit Diagram Connector Location BMS ECU Connector And Terminal Function BMS ECU Terminal Function A Connector [B01-A] (35 Pin) - Voltage Measurement Connector Pin no.DescriptionCo ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Hub / Knuckle Repair procedures

Replacement 1. Loosen the wheel nuts slightly. Raise the vehicle, and make sure it is securely supported. 2. Remove the front wheel and tire (A) from front hub. Tightening torque: 88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft) Be careful not to da ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Description and Operation

Description The system temperature is calculated by the BMS based on 8 temperature sensor signals. And the cooling fan is conrolled in 9 steps to maintain the normal temperature of high voltage battery system. The air-cooling method is applied in the cooling system where indoor air is used ...
Copyright © www.ksoulev.com 2020-2021