- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Tire Pressure Monitoring System / TPMS Receiver Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Suspension System / Tire Pressure Monitoring System / TPMS Receiver Repair procedures

Replacement

When the receiver first arrives for replacement:
a. | It will be in Virgin State.
b. | It will not be configured for any specific platform.
c. | It will not have any sensor ID''s memorized.

It is important to make sure that the correct receiver is used to replace the faulty part i.e. it must be Low Line and not High Line in order to have the correct inflation warning thresholds set.

1. | Disconnect vehicle battery.

2. | Remove the crash pad garnish. (Refer to BD group - "Crash Pad")

3. | Remove the receiver with bracket.

4. | Install in the reverse order of removal.

5. | Re-connect battery and turn Ignition on.

6. | After replacing the receiver, learn by using self-diagnosis device(GDS).

[Wheel Sensor ID Writing (Wireless) initialization]

[Wheel Sensor ID Writing (Wireless) 1]

[Wheel Sensor ID Writing (Wireless) 2]

Diagnosis procedure by using diagnostic device

As manual for diagnosis methods by using diagnosis device, the main contents are as follows:

1. | Connect self-diagnosis connector(16pins) located in the lower of driver side crash pad to self-diagnosis device, and then turn the self-diagnosis device after key is ON.

2. | Select the "vehicle model" and "TPMS" on GDS vehicle selection screen, then select OK.

[System Identification (Wireless)]

[Sensor ID Writing (Wireless)]

[VIN input initialization]

[Vehicle name input initialization]

[Sensor Status initialization]

[Register Sensor initialization]

• | Write ID Read ID and be sure to check are the same.
• | After registering successfully sensor "Sensor Wireless Information" by the execution determines whether the sensor is working properly.

##### TPMS Receiver Description and Operation

Description 1. Mode (1) Virgin State • The receiver as a sole part is shipped in this state. Replacement parts should therefore arrive in this state. • In this state, there ...

##### Steering System

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Smart Key Unit Repair procedures

Inspection Smart Key Unit – Refer to Smart key System - "Smart key Diagnostic" Smart Key Switch – Refer to Smart key System - "Smart key Diagnostic" Antenna – Refer to Smart key System - "Smart key Diagnostic" Trunk Lid Open Switch 1. Check for continuity ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Height Adjust Components and Components Location

Component Location 1. Height adjust ...
Copyright © www.ksoulev.com 2020-2021