- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Hood / Hood Latch Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Hood / Hood Latch Repair procedures

Replacement

1. | Remove the charge door handle (A).

2. | Loosen the front bumper upper cover mounting bolts and clips.

3. | Gently lift the bumper upper cover.

4. | Loosen the screw (B), and then remove the front bumper upper cover (A).

5. | Loosen the bolts, and then remove the hood latch assembly (B).

6. | Disconnect the hood latch cable (A) and remove the hood lower latch assembly (B).

7. | Install in the reverse order of removal.
• | Make sure that the hood latch release cable is connected properly.
• | Make sure that the hood locks/unlocks and opens/closes properly.
• | Adjust the latch alignment.

##### Hood Latch Components and Components Location

Component Location 1. Hood lower latch assembly ...

##### Interior Trim

...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Turn Signal Lamp Repair procedures

Removal Door Mirror Turn Signal Lamp 1. Disconnect the negative (-) battery terminal. 2. Remove the mirror holder (A) from the outside mirror assembly. 3. Remove the door mirror cover (A). Be careful not to damage the fixing clip. 4. Loosen the mirror ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Front Bumper Cover Components and Components Location

Component Location 1. Front bumper cover ...
Copyright © www.ksoulev.com 2020-2021