- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: Body Side Moulding / A Pillar Garnish Repair procedures

Kia Soul EV (PS EV) 2015-2020 Service Manual / Body (Interior and Exterior) / Body Side Moulding / A Pillar Garnish Repair procedures

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage.
• | Take care not to scratch the body surface.

1. | After loosening the mounting screw, remove the A pillar garnish (A) using a screw driver.
• | Replace the A pillar garnish with a new one.

2. | Install in the reverse order of removal.
• | Replace any damaged clips.

##### Fender Garnish Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Front Wheel Guard Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protec ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Movable Glass Repair procedures

Replacement 1. Completely open the movable glass using the panorama sunroof switch. 2. Remove both sides of the decoration cover (A) by pulling it in the direction of the arrow. 3. Completely close the movable glass using the panorama sunroof switch. 4. Adjust the height of the glas ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: General Safety Information and Caution

Safety Precaution Since electric vehicles contain high voltage batteries, mishandling the high voltage system or vehicle may lead to a serious accident, including electric shock and electric leakage. • Be sure to shut o ...
Copyright © www.ksoulev.com 2020-2021