- Soul EV Manuals
- Owners
- Service
- New
- Top
- Sitemap
- Search

# Kia Soul EV: High Voltage Battery Control System / Main Relay Specifications

Kia Soul EV (PS EV) 2015-2020 Service Manual / EV Battery System / High Voltage Battery Control System / Main Relay Specifications

Specification

Item | Specification
ON | Rated Voltage (V) | 450
Rated Ampere (A) | 200
Voltage Drop (V) | Less than 0.1 (200A)
Coil | Operation Voltage (V) | 12
Resistance (?) | 21.6 ~ 26.4 (20°C)

Item | Specification | Note
Main Relay Fixing Status | NO | Checkable by GDS
Main Relay Switch (-) Resistance (?) | ? | Checkable by multi tester
Main Relay Operation Beep | "Clicking" | Checkable by GDS and SST
Coil Resistance (?) | 21.6 ~ 26.4 (20°C) | Checkable by multi tester

##### Battery Management System (BMS) ECU Repair procedures

Inspection C-CAN Terminating Resistance Inspection (Multi Purpose Check Connector) 1. Turn the ignition OFF. 2. Measure the resistance between pins No. 20 and No. 17 of multi purpose check ...

##### Main Relay Description and Operation

Description Main Relay is installed in the Power Relay Assembly (PRA) and it controls the high voltage line. It connects the power between the high voltage battery pack and the high voltage joint ...

##### Other information:

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Components and Components Location

Component Location 1. Cluster assembly2. Seat belt switch3. Brake fluid level warning switch4. Parking brake switch5. Door switch6. Tailgate switch7. Wheel speed sensor8. ABS ECU ...

### Kia Soul EV (PS EV) 2015-2020 Service Manual: Main Crash Pad Assembly Repair procedures

Replacement • Put on gloves to protect your hands. • When prying with a flat-tip screwdriver, wrap it with protective tape, and apply protective tape around the related parts, to prevent damage. • Us ...
Copyright © www.ksoulev.com 2020-2021